

Plug and play, integrated auto detecting, auto configuration, and auto firmware upgrade

Integrated OMCI and TR069 remote configuration and maintenance function.

Support rich QinQ VLAN, DHCP Server/Relay and IGMP/MLD snooping multicast feature.

Support fiber transceiver diagnostic monitoring, fiber transmitter disable remotely.

Fully compatibility with OLT based on Broadcom chipset etc.

Support 802.11n WiFi (2T2R) function.

Support NAT, Firewall function.

Support IPv4 and IPv6 dual stack.

 ONT-4GE-2VWX GPON ONT Manual

 ONT-4GE-2VWX GPON ONT/HGU

 Introduction

 ONT-4GE-2VWX is designed for fulfilling FTTH (Fiber To The Home) and triple play service

 demand of fixed network operators. It is developed wholly by Guangzhou V-Solution. The box is

 based on the mature Gigabit GPON technology, which has high ratio of performance to price, and

 the technology of 802.11n WiFi (2T2R), Layer 2&3 and high quality VoIP as well. It is highly

 reliable and easy to maintain, with guaranteed QOS for different service. And It is fully compliant

 with technical regulations such as ITU-T G.984.x and technical requirement of GPON Equipment

 (V2.1 and above version) from China Telecom.

 ONT-4GE-2VWX

 Special features

 

 technology.

 

 

 

 

 

 

 



Integrated line testing compliant with GR-909 on POTS.

 ONT-4GE-2VWX GPON ONT Manual

 

  The WAN port supports bridge, router and bridge/router mixed mode.

 Technical parameters

|  |  |
| --- | --- |
| Technical items | Descriptions |
| Chipsets | BCM68380F |
| Optical interface | 1 GPON interface, SC single-mode/single-fiber, Downstream rate 2.5Gbps, |
| Upstream rate 1.25Gbps |
| Optical Wavelength | Tx 1310nm, Rx 1490nm |
| Optical interface | SC/PC |
| RX sensitivity | < -25dBm @ 1490nm |
| WLAN | Compliant with IEEE802.11b/g/n, 300Mbps, 2T2R |
| one internal antenna and one external antenna |
| WLAN throughput | 100Mbps @ 40users, 1518bytes, no-encryption |
| 107Mbps @ 40users, 512bytes, encryption |
| LAN interface | 4\*10/100Mbps |
| Auto adaptive Ethernet interfaces, Full/Half Duplex, RJ45 connectors |
| Router throughput | Upstream: >390Mbps @ 1518bytes, Downstream: >390Mbps @ 1522bytes |
| POTS interface | 2 FXS, RJ11 connectors |
| Indicators | 14 indicators |
| DC power supply | +12V@1A, external AC-DC power adaptor |
| Button | RST, Power, WiFi, WPS, Pair |
| Power | ≤ 10W |
| consumption |
| Operating | Operating temp: -5 ~ +55 | ℃ | ,Operating humidity: 10~90% (non-condensed) |
| condition |
| Storing condition | Storing temp: -30 ~ +60 | ℃ | ,Storing humidity:10~90%(non-condensed) |
| Dimension | 205mm\*138mm\*50mm(length\*width\*height) |
| Net weight | 0.4Kg |

 Data Service Functions

 1) Full speed non-blocking switching.

 2) 2048 MAC address table.

 3) 64 full range 4095 VLAN ID

 4) Support VLAN QinQ, transparent, tag, translation, trunk, etc.

 5) Integrated port monitoring, port mirroring, port rate limiting, port SLA, etc.

 6) Support auto polarity detection of Ethernet ports (AUTO MDIX).

 7) Integrated IEEE802.1p QoS with four level priority queues.

 8) Support IPv4 IGMP snooping and IPv6 MLD snooping.

 9) Support bridging, router and bridging/router mixed mode.



 ONT-4GE-2VWX GPON ONT Manual

 POTS Service Functions

 1) Call protocol: SIP (IMS compatible), seamless compatible with all popular call agent.

 2) Integrate heartbeat function and support active/standby call agent.

 3) Voice coding: ITU-T G.711/G.723.1(5.3K/6.3Kbit/s)/G.729, auto-negotiate with call agent.

 4) Echo cancellation exceeding ITU-T G.165/G.168-2002, up to 128ms tail length.

 5) Support high/low speed fax/Modem, bypass fax, and T38 fax.

 6) Support RFC2833 and redundant RFC2833, difference rings, MD5 authentication, call

 forward, call waiting, hot-line call, alarm clock, and all kinds of value-added voice service.

 7) Multi-party conferencing.

 8) Line testing according to GR-909.

 9) IP address assignment: dynamic PPPoE/DHCP Client and static IP.

 10) Support WEB, CLI, TR069.

 11) Integrated OAM, XML, DHCP option 66 & 67 for auto configuration and firmware upgrade.

 12) Call loss is less than 0.01%.

 WiFi service

 1) Integrated 802.11b/g/n, 300Mbps, 2T2R.

 2) Support 128 connections.

 3) Support WEP and WPA/WPA2 security protocols.

 Application chart

 Key Words:

 GPON ONT, GPON HGU, WiFi ONT, GPON ONU

 Compatible with HUAWEI M5680T OLT

 Compatible with ZTE C300 OLT

 Compatible with Fiberhome AN5516 OLT

 Based on BCM6838



 ONT-4GE-2VWX GPON ONT Manual