

Plug and play, integrated auto-detecting, auto-configuration, and auto firmware upgrade,

Integrated OMCI/TR069 remote configuration and maintenance function.

Support rich QinQ VLAN function and IGMP Snooping multicast feature.

Functions like transceiver diagnostic monitoring, transmitter disable, etc.

Built-in bridging or router mode.

Fully compatibility with OLT based on Broadcom/Broadlight.

 ONT-1GEX GPON ONT Manual

 ONT-1GEX 1GE GPON ONT

 Introduction

 ONT-1GEX is a low density GPON ONT designed for fulfilling FTTH request of telecom

 operators, internet access of SOHO people and renovation request of GPON+EOC infrastructure

 of cable TV operators. This product is based on the stable and mature Gigabit GPON technology,

 which has high performance/price ratio. Its GPON MAC chip is the newest generation SOC -

 BCM6838 from world famous xPON IC vendor - Broadcom. It is highly reliable and easy to

 maintain, with guaranteed QoS. And it is fully compliant to technical regulations such as

 ITU~T984.X and technical requirement of GPON Equipment (V1.2 and above version) from China

 Telecom.

 ONT-1GEX

 Special features

 

 etc.

 

 

 

 

 

 Technical parameter

|  |  |
| --- | --- |
| Technical items | Descriptions |
| Upstream PON | 1 GPON interface, SC single-mode/single-fibre, Upstream 1.244Gbps, |
| Interface | Downstream 2.488Gbps. |
| GPON MAC | BCM6838 SOC from Broadcom. |
| Wavelength | Tx 1310nm, Rx 1490nm. |
| Optical interface | SC/PC connector. |
| Downstream LAN | 1x 10/100/1000Mbps auto adaptive Ethernet interface, Full Duplex/Half |
| interface | Duplex, RJ45 connector. |

 Page 1



 ONT-1GEX GPON ONT Manual

|  |  |  |
| --- | --- | --- |
| Indicators | 5 indicators, for status of power, Los status of PON port, Register status of |  |
| PON port, Link status of Giga-Ethernet port, Active status of Giga-Ethernet |
| port. |
| DC power supply | +12V@0.5A, external AC/DC power adaptor |
| Power | ≤5W |
| consumption |
| Operating | Operating temp: ~5 ~ +55 | ℃ | , operating humidity:10~90% (non-condensed) |
| condition |
| Storing condition | Storing temp: ~30 ~ +60 | ℃ | , storing humidity:10~90% (non-condensed) |
| Device Dimension | 115mm\*75mm\*28mm (length\*width\*height) |
| CANTON | Internal Canton: 20.5mm\*16mm\*5.5mm |
| Package: 590mm\*410mm\*325mm |
| Dimension |
| 40PCS/CTN |
| Net weight | 0.24Kg |
| **Application ch** | **rt** |
| **Ordering infor** | **ation** |
| Product model | GE | Work temperature | Product Form |
| ONT-1GEX | 1 | ~5 ~ +55℃ | Plastic casing |

 Page 2